(footprint "TINY2040"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "2688779e-783b-45b2-aa2e-fb5875f29011")
		(effects
			(font
				(size 0.787402 0.787402)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TINY2040"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "74243dfb-1d03-4859-8798-b42494ec651a")
		(effects
			(font
				(size 0.787402 0.787402)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "137b5d4c-f799-4022-a7ef-2393607ff76d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c7b83eaa-85fe-46d7-a4c9-574bbc8947d7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.98 3.92579)
		(end -0.98 -3.90579)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f6cbbb89-9470-4d46-93df-579e77db6189")
	)
	(fp_line
		(start -0.687106 -4.61289)
		(end -0.292894 -5.00711)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e9799d77-bf49-4067-b72b-37a55696b8d7")
	)
	(fp_line
		(start -0.292894 5.02711)
		(end -0.687106 4.63289)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "65a21523-33dd-4288-b3b9-d78782a43c85")
	)
	(fp_line
		(start 0 -5.71421)
		(end 0 -8.6)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e65b9940-a7f8-4b84-b655-9e9449b2cead")
	)
	(fp_line
		(start 0 8.6)
		(end 0 5.73421)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f6a2f223-cf52-425e-881c-5a4403f83148")
	)
	(fp_line
		(start 0.4 -9)
		(end 19.92 -9)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "85a275e0-4712-42fa-8ce2-9e932c345d03")
	)
	(fp_line
		(start 19.92 9)
		(end 0.4 9)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "883a851b-efa3-4f3e-8c77-23676f10c87a")
	)
	(fp_line
		(start 20.32 8.6)
		(end 20.32 -8.6)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b319fdc5-1d04-45b9-a755-67ef05135236")
	)
	(fp_arc
		(start -0.98 -3.90579)
		(mid -0.903879 -4.28847)
		(end -0.687106 -4.61289)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "326ae578-7013-46ce-a5c6-b66a2fc1d135")
	)
	(fp_arc
		(start -0.687106 4.63289)
		(mid -0.903878 4.30847)
		(end -0.98 3.92579)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "89ba8e95-e94d-4b59-9f95-44cb40bce82e")
	)
	(fp_arc
		(start -0.292894 5.02711)
		(mid -0.076122 5.35153)
		(end 0 5.73421)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b4018e83-5620-40aa-98a5-0267176bbe33")
	)
	(fp_arc
		(start 0 -8.6)
		(mid 0.117157 -8.882843)
		(end 0.4 -9)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "79dd59dc-d4d8-408e-a831-1bd53dfd7dd7")
	)
	(fp_arc
		(start 0 -5.71421)
		(mid -0.076121 -5.33153)
		(end -0.292894 -5.00711)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4be12d2f-428b-4ae6-a0ab-5c9485754149")
	)
	(fp_arc
		(start 0.4 9)
		(mid 0.117157 8.882843)
		(end 0 8.6)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f0c6ce72-2d65-4708-b745-87d57d7d0d5d")
	)
	(fp_arc
		(start 19.92 -9)
		(mid 20.202843 -8.882843)
		(end 20.32 -8.6)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f8097dd9-b0dc-43c5-83a8-6c8764144529")
	)
	(fp_arc
		(start 20.32 8.6)
		(mid 20.202843 8.882843)
		(end 19.92 9)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a545fb0d-cb8f-41ee-a070-beba12bfbda3")
	)
	(fp_line
		(start 0.7 -6.3)
		(end 16.62 -6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "f144a41f-3703-4af2-9e1e-d7b59888a851")
	)
	(fp_line
		(start 16.62 6.3)
		(end 0.7 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "efca9d0a-d96d-4e78-8f94-1212108b9247")
	)
	(fp_line
		(start 17.62 -5.3)
		(end 17.62 5.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "3fa393f2-56db-4a49-8604-e0ea5eb1c878")
	)
	(fp_arc
		(start 16.62 -6.3)
		(mid 17.327107 -6.007107)
		(end 17.62 -5.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "9a002857-6f63-4fb7-9a57-4e04f1ce7335")
	)
	(fp_arc
		(start 17.62 5.3)
		(mid 17.327107 6.007107)
		(end 16.62 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "1ca087e7-4176-40de-adce-328c14104c76")
	)
	(fp_line
		(start -2.175 -4.32)
		(end -2.175 4.32)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b724e1ad-869a-4317-a020-7d8f8de2e405")
	)
	(fp_line
		(start -2.175 -4.32)
		(end 5.645 -4.32)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5ef26fa8-15d3-469b-84ee-ca7f40a93b4c")
	)
	(fp_line
		(start 1.225 -4.32)
		(end -0.375 -4.32)
		(stroke
			(width 0.01)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7067cd3d-e41b-4e77-b8d5-dd775fa372b3")
	)
	(fp_line
		(start 5.645 -4.32)
		(end 3.555 -4.32)
		(stroke
			(width 0.01)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6b180929-cfe1-41f2-b2a1-7107f1127878")
	)
	(fp_line
		(start 5.645 -4.32)
		(end 5.645 4.32)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1c03bd52-d761-43dd-be5e-9be53e44c8aa")
	)
	(fp_line
		(start 5.645 4.32)
		(end -2.175 4.32)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "999a51f3-cf01-4dd0-9b40-e9a5ee0fa626")
	)
	(fp_line
		(start 5.645 4.32)
		(end 3.555 4.32)
		(stroke
			(width 0.01)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4756eee6-faf6-4581-992a-dddb799799ff")
	)
	(fp_line
		(start 5.655 -4.32)
		(end 5.645 -4.32)
		(stroke
			(width 0.01)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2ddb1039-9ceb-4fdd-a6bb-9eb25a41e59a")
	)
	(fp_line
		(start 5.655 4.32)
		(end 5.645 4.32)
		(stroke
			(width 0.01)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "70a3d4be-f879-4b37-9c78-67155e66c88b")
	)
	(pad "0" smd roundrect
		(at 1.27 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "836208e1-cacc-4dd7-a7bf-5fcf9172c4a2")
	)
	(pad "1" smd roundrect
		(at 3.81 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "b99a77c1-b06a-403d-a518-6c2d332f474d")
	)
	(pad "2" smd roundrect
		(at 6.35 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "4c67c99c-3671-461e-a791-591772e126f5")
	)
	(pad "3" smd roundrect
		(at 8.89 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "8d498076-9258-43ee-9822-fc14b7818a0b")
	)
	(pad "3V3" smd roundrect
		(at 6.35 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "ca3f498a-afca-40c3-9b85-c6c5721ff60c")
	)
	(pad "4" smd roundrect
		(at 11.43 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "1a0b70d7-12b3-4170-9a0b-95bbb252d868")
	)
	(pad "5" smd roundrect
		(at 13.97 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "3975bee7-3dbf-4cad-8953-f0554b3e08e0")
	)
	(pad "5V" smd roundrect
		(at 1.27 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "f7a19bc5-d1b2-46a1-a852-e00350316b6a")
	)
	(pad "6" smd roundrect
		(at 16.51 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "c41ae3b8-6a4c-4f27-8e3e-db1439176639")
	)
	(pad "7" smd roundrect
		(at 19.05 -8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "b9312c4d-4ec3-4426-a9f4-767135c0d58b")
	)
	(pad "A0" smd roundrect
		(at 16.51 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "820316b5-a04f-4c64-b5e2-958640b5431f")
	)
	(pad "A1" smd roundrect
		(at 13.97 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "6a15232f-5b2a-4af1-a053-6300c1cf1b7a")
	)
	(pad "A2" smd roundrect
		(at 11.43 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "dc2b97df-40be-4a5b-8f3e-33b2e7ceca77")
	)
	(pad "A3" smd roundrect
		(at 8.89 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "1832c307-69f8-4964-b803-353926fd444f")
	)
	(pad "GND1" smd roundrect
		(at 3.81 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "a7e3ef1c-c67d-4bd8-9b2d-cbe7d603a8a1")
	)
	(pad "GND2" smd roundrect
		(at 19.05 8.17)
		(size 1.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "31f2724d-3410-4149-a98b-55f499b075d9")
	)
	(pad "GND3" smd roundrect
		(at 19.49 0)
		(size 3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "2dff7709-d244-4111-8c07-fbfaaafe841e")
	)
	(pad "SWCLK" smd roundrect
		(at 19.49 2.54)
		(size 3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "90b00094-f666-49ce-88ef-e6753661df2d")
	)
	(pad "SWDIO" smd roundrect
		(at 19.49 -2.54)
		(size 3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(solder_mask_margin 0.102)
		(uuid "68001a20-177b-4692-9fc5-7fdcfc0c5cef")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "4d4fa5a4-10e5-4fee-9c02-7c319c0b173d")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 17.4 -6.4) (xy 20 -6.4) (xy 20 -3.8) (xy 17.4 -3.8)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "6dd6c51e-529a-4579-9a82-9f0d6f37224b")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 17.4 3.8) (xy 20 3.8) (xy 20 6.4) (xy 17.4 6.4)
			)
		)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/Tiny2040.step"
		(offset
			(xyz 10.16 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -90)
		)
	)
)
